## System Logging

The event log kept by the Intel® PRO/Wireless 2011B LAN Access Point allows you to log events that you select.

1. Select Set Event Logging Configuration from the Main Menu .
2. Set Any Event Logging to Enabled to log all events. Specify the events that do not require logging when disabling Any Event Logging . Use SPACE BAR or LEFT/RIGHT-ARROW keys to toggle between Enabled and Disabled :

Any Event Logging | Logs all events listed in the screen.
Security Violations | ACL filter or administrative password access violations.
MU State Changes | Allows logging all client computer state changes.
WNMP Events | WNMP events such as computers using WNMP.
Serial Port Events | Serial port activity.
AP-AP Msgs | Access point-to-access point communication.
Telnet Logins | Telnet sessions for monitoring and administration.
System Events | Internal use only.
Ethernet Events | Events such as packet transmissions and errors.

3. Verify that the values reflect the network environment. Change them as needed.
4. Select OK or Save to register settings.
5. Select Save ALL APs-[F2] to save the Event Logging Configuration information to all access points with the same SSID. This option saves the configuration changes for the current access point and sends two messages to all other access points on the Known APs table to update their configuration and reset after the configuration has been modified. You can perform this option only among the same hardware platforms and firmware versions.

Copyright © 2002 Intel Corporation. Legal Information