# Intel® PRO/Wireless 5000 LAN Access Point
Configuration Management System Help File

This file contains information on the screens and parameters accessible through the browser-based Access Point Configuration Management System.

The screens covered are the following:

Access Control List
Client History
Client Statistics
File Transfer
Ethernet Statistics
Express Setup
Configuration
Radio 802.11a
Radio 802.11b
Ethernet Setup
Radio Statistics
SNMP Agent
SNTP Server
Change Login Info
WEP Settings

## Access Control List 802.11a/802.11b

## ACL Mode

Description | How to use the Access Control List (ACL): "Disabled" disables the Access Control List. "Enabled" causes stations in the list with "Allowed" attribute set to "No" to be rejected when attempting to associate with the Access Point. "Strict" allows stations that are in the list with "Allowed" attribute set to "Yes" to associate with the Access Point, but only using the WEP mapping as indicated.
Valid Range | Enabled, Disabled, Strict.

### Access Control List

Each entry is a station identified by its MAC address. The station has two attributes: "Allowed" and "WEP map". The user may select one or more entries of this list to be deleted by pressing the "Delete" button.

### Allowed

Description | The meaning of this attribute depends on the setting for "ACL Mode", as follows: If "ACL Mode" is set to "Strict", and "Allowed" is set to "Yes", this indicates that the station is allowed to associate with the Access Point, but only with WEP mapping as indicated. All other stations are disallowed to associate with the Access Point. If "ACL Mode" is set to "Enabled", and "Allowed" is set to "No", this station is not allowed to associate with the Access Point (WEP mapping does not matter). All other stations are allowed to associate with the Access Point.
Valid Range | Yes, No.

### WEP Map

Description | Indicates how the station uses WEP keys. If "Allowed" attribute is set "No", then "WEP map" is set "* (any)", i.e. it doesn't matter.
Valid Range | 1 (WEP Key 1), 2 (WEP Key 2), 3 (WEP Key 3), 4 (WEP Key 4), d (default WEP Key), * (any).

### MAC Address

Description | The MAC address of the station.
Valid Range | MAC address of the form nn:nn:nn:nn:nn:nn

### Edit

Description | Button to bring into editable fields the currently selected entry in Access Control List.

### Delete

Description | Button to delete the selected entries from the Access Control List.

### Modify

Description | Button to replace the currently selected entry in Access Control List with the one from editable fields.

### Add

Description | Button to add a new entry to the Access Control List.

### Restart AP

Description | Button for restarting the Access Point. When Restart AP is pressed, the Access Point requests user confirmation.

### Apply

Description | Button for applying new settings. Most settings become effective only after the Access Point is restarted. When Apply is pressed, the Access Point requests user confirmation.

## Client History 802.11a/802.11b

The Client History is a list of entries corresponding to those stations which attempted at least to authenticate with the Access Point. Each entry has the following fields:

### MAC Address

Description | The MAC address of the station.
Valid Range | MAC address of the form nn:nn:nn:nn:nn:nn

### Latest Activity

Description | The time when the station performed the last packet transfer with the Access Point.
Valid Range | N/A.

### State

Description | The state of the station when this page is accessed.
Valid Range | Assoc (associated), Auth (authenticated), Away (not authenticated).

### Tx Packets

Description | The number of packets sent by the Access Point to the station.
Valid Range | Positive integer (0 included).

### Rx Packets

Description | The number of packets received by the Access Point from the station.
Valid Range | Positive integer (0 included).

### Refresh

Description | Button to refresh the Client History.

When the user clicks the MAC address of a station presented in the Client History, the Access Point shows the "Client Station Log" page for that station.

## Client Statistics 802.11a/802.11b

### MAC Address

Description | The MAC address of the station.
Valid Range | MAC address of the form nn:nn:nn:nn:nn:nn

### Association ID

Description | The Association ID assigned by the Access Point to the station, if the station is in the "Assoc" state.
Valid Range | 1 - 2007

### State

Description | The state of the station when this page is accessed.
Valid Range | Assoc (associated), Auth (authenticated), Away (not authenticated).

### Current Rate

Description | The current data transmission rate.
Valid Range | For 802.11a clients, one of the following rates: 6, 9, 12, 18, 24, 36, 48, 54 Mbps. For 802.11b clients, one of the following rates: 1, 2, 5.5, 11 Mbps.

### Operational Rates

Description | The data transmission rates in common between the Access Point and the station.
Valid Range | For 802.11a clients, a subset of the following rates: 6, 9, 12, 18, 24, 36, 48, 54 Mbps. For 802.11b clients, a subset of the following rates: 1, 2, 5.5, 11 Mbps.

### Signal Strength

Description | The current index of radio signal quality.
Valid Range | 0 - 100%.

### Latest Activity

Description | The time when the station performed the last packet transfer with the Access Point.
Valid Range | N/A.

### Transmit Statistics, Packets OK

Description | The number of good packets received by the Access Point to send to the station.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Total Errors

Description | The number of packets with errors received by the Access Point to send to the station.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Max Retry Packets

Description | The number of times RTS and data packets sent by the Access Point to the station reached the maximum retry number.
Valid Range | Positive integer (0 included).

### Transmit Statistics, RTS Retries

Description | The number of times RTS packets sent by the Access Point to the station had to be retried at least once.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Data Retries

Description | The number of times data packets sent by the Access Point to the station had to be retried at least once.
Valid Range | Positive integer (0 included).

### Receive Statistics, Packets OK

Description | The number of good packets received by the Access Point from station.
Valid Range | Positive integer (0 included).

### Receive Statistics, Total Errors

Description | The number of packets with errors received by the Access Point from the station.
Valid Range | Positive integer (0 included).

### Receive Statistics, WEP Errors

Description | The number of packets with WEP errors received by the Access Point from the station.
Valid Range | Positive integer (0 included).

### Deauthenticate

Description | Button to cause the Access Point to send a deauthentication notification packet to the station.

### Disassociate

Description | Button to cause the Access Point to send a disassociation notification packet to the station.

### Diagnosic Info

Description | Button to show Access Point internal information that may be useful for troubleshooting.

### Clear Statistics

Description | Button to clear the station statistics.

### Refresh Statistics

Description | Button to refresh the station statistics.

## Firmware Update

### TFTP Server Address

Description | The IP address of the host machine that has a TFTP server configured for file transfer to the Access Point.
Valid Range | Valid IP address format.

### File Path

Description | The path needed on the TFTP server for the Access Point to access files on the TFTP server. Depending on how the TFTP server is configured, this path may not be needed.
Valid Range | 0 - 255 characters

### File Name

Description | The file name on the TFTP server for the file to be transferred to the Access Point.
Valid Range | 1 - 255 characters

### Update Firmware

Description | Button to start TFTP file transfer to update the AP firmware.

### Restart AP

Description | Button for restarting the Access Point. When Restart AP is pressed, the Access Point requests user confirmation.

## Ethernet Statistics

### MAC Address

Description | The MAC address of the Access Point.
Valid Range | MAC address of the form nn:nn:nn:nn:nn:nn

### Speed

Description | The speed of the Ethernet interface.
Valid Range | Auto, 10BaseTHalfDuplex, 100BaseTHalfDuplex, 10BaseTFullDuplex, 100BaseTFullDuplex.

### Transmit Statistics, Unicast Packets

Description | The number of unicast packets transmitted to the wired network.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Multicast Packets

Description | The number of multicast packets transmitted to the wired network.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Total Bytes

Description | The number of bytes transmitted to the wired network.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Wrong Packets

Description | The number of packets received from the radio that contained errors.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Max Retry Packets

Description | The number of times packets sent to the wired network reached the maximum retry number.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Collisions

Description | The number of packet collisions that occurred through this interface.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Underrun Packets

Description | The number of packets received from the radio which were discarded because the Ethernet interface was starved for data.
Valid Range | Positive integer (0 included).

### Receive Statistics, Unicast Packets

Description | The number of unicast packets received from the wired network.
Valid Range | Positive integer (0 included).

### Receive Statistics, Multicast Packets

Description | The number of multicast packets received from the wired network.
Valid Range | Positive integer (0 included).

### Receive Statistics, Total Bytes

Description | The number of bytes received from the wired network.
Valid Range | Positive integer (0 included).

### Receive Statistics, Wrong Packets

Description | The number of packets received from the wired network that presented errors.
Valid Range | Positive integer (0 included).

### Receive Statistics, CRC Errors

Description | The number of packets with CRC errors received from the wired network.
Valid Range | Positive integer (0 included).

### Receive Statistics, Overrun Packets

Description | The number of packets received from the wired network that were discarded because the Access Point had a temporary overload of packets to handle.
Valid Range | Positive integer (0 included).

### Receive Statistics, Too Short Packets

Description | The number of packets received from the wired network that were shorter than the minimum packet size of 64 bytes
Valid Range | Positive integer (0 included).

### Receive Statistics, Too Long Packets

Description | The number of packets received from the wired network that were larger than the maximum packet size of 1518 bytes.
Valid Range | Positive integer (0 included).

### Receive Statistics, Truncated Packets

Description | The number of packets received from the wired network that were corrupt or incomplete.
Valid Range | Positive integer (0 included).

### Clear Statistics

Description | Button to clear the Ethernet statistics.

### Refresh Statistics

Description | Button to refresh the Ethernet statistics.

## Express Setup

### Access Point Name

Description | A descriptive name for the Access Point.
Valid Range | 1 - 32 characters
Default | WDAP5000

### Default IP Address

Description | The static IP address of the Access Point (effective if DHCP usage is disabled or DHCP server is not available).
Valid Range | Valid IP address format.
Default | 192.0.2.1

### Default Subnet Mask

Description | The static subnet mask of the Access Point (effective if DHCP usage is disabled or DHCP server is not available).
Valid Range | Valid IP address format. |
Default | 255.255.0.0

### Default Gateway

Description | The IP address of the default gateway (effective if DHCP usage is disabled or DHCP server is not available).
Valid Range | Valid IP address format.
Default | None (no default gateway)

### DHCP

Description | DHCP (Dynamic Host Configuration Protocol) usage.
Valid Range | Enabled, Disabled.
Default | Disabled

### Help URL

Description | The URL of the Help system file.
Valid Range | Valid URL format.
Default | Empty string (Help not installed).

### SSID 802.11a

Description | SSID (Service Set Identifier) of 802.11a service set (driven by radio 802.11a).
Valid Range | 1 - 32 characters.
Default | 101

### SSID 802.11b

Description | SSID (Service Set Identifier) of 802.11b service set (driven by radio 802.11b).
Valid Range | 1 - 32 characters.
Default | 101

### Restart AP

Description | Button for restarting the Access Point. When Restart AP is pressed, the Access Point requests user confirmation.

### Apply

Description | Button for applying new settings. Most settings become effective only after the Access Point is restarted. When Apply is pressed, the Access Point requests user confirmation.

## Configuration

### Regulatory Domain

Description | The name of the regulatory area the channels of the Access Point radio are configured to work in. This determines the channel and frequencies used by the Access Point and the clients. The Regulatory Domain for the Access Point and clients must match in order for them to work together.
Valid Range | Americas, Europe, Japan, Asia-Pacific.

### MAC Address

Description | The MAC (Media Access Control) address used by the Access Point.
Valid Range | MAC address of the form nn:nn:nn:nn:nn:nn

### Current IP Address

Description | The IP address currently used by the Access Point. If DHCP is enabled and available, this is the dynamic address assigned by the DHCP server, otherwise this is the Default IP Address.
Valid Range | Valid IP address format.

### Current Subnet Mask

Description | The subnet mask currently used by the Access Point. If DHCP is enabled and available, this is the dynamic subnet mask assigned by the DHCP server, otherwise this is the Default Subnet Mask.
Valid Range | Valid IP address format.

### Access Point Name

Description | The name of the Access Point.
Valid Range | 1 - 32 characters.
Default | WDAP5000

### Default IP Address

Description | The static IP address of the Access Point (effective if DHCP usage is disabled or DHCP server is not available).
Valid Range | Valid IP address format.
Default | 192.0.2.1

### Default Subnet Mask

Description | The static subnet mask of the Access Point (effective if DHCP usage is disabled or DHCP server is not available).
Valid Range | Valid IP address format.
Default | 255.255.0.0

### Default Gateway

Description | The IP address of the default gateway (effective if DHCP usage is disabled or DHCP server is not available).
Valid Range | Valid IP address format.
Default | None (no default gateway)

### DHCP

Description | DHCP (Dynamic Host Configuration Protocol) usage.
Valid Range | Enabled, Disabled.
Default | Disabled

### Help URL

Description | The URL of the AP Help file.
Valid Range | Valid URL format.
Default | Empty string (Help not installed).

### Restore Default Configuration

Description | Button for restoring factory settings. Most settings become effective only after the Access Point is restarted. When Restore Default Configuration is pressed, the Access Point requests user confirmation.

### Restart AP

Description | Button for restarting the Access Point. When Restart AP is pressed, the Access Point requests user confirmation.

### Apply

Description | Button for applying new settings. Most settings become effective only after the Access Point is restarted. When Apply is pressed, the Access Point requests user confirmation.

## Radio 802.11a

### BSSID

Description | The BSSID (Basic Service Set Identifier) of the radio 802.11a.
Valid Range | MAC address of the form nn:nn:nn:nn:nn:nn

### Authentication Type

Description | The type of authentication algorithm required to be used by a client station attempting to authenticate with the Access Point. "Shared" authentication requires the Access Point and stations to use the authentication key indicated by the "Default WEP Key" setting of the "WEP Settings 802.11a" page. That key must be defined in order for “Shared” to be used.
Valid Range | Open, Shared.
Default | Open.

### SSID

Description | Service Set Identifier String. The Access Point broadcasts this string in its beacons.
Valid Range | 1 - 32 characters.
Default | 101

### Antenna Pattern

Description | The pattern of the radio antenna.
Valid Range | Omni, half circle front.

### Radio Channel

Description | The frequency at which the radio operates.
Valid Range | 36 [5.18 GHz], 40 [5.20 GHz], 44 [5.22 GHz], 48 [5.24 GHz], 52 [5.26 GHz], 56 [5.28 GHz], 60 [5.30 GHz], 64 [5.32 GHz].

### Transmit Power

Description | The radio transmission power level.
Valid Range | MAX, 50%, 25%. 12%. MIN.

### Fragment Threshold

Description | The Fragmentation threshold is the size at which packets will be fragmented and transmitted piecemeal instead of all at once.
Valid Range | 256 – 2346

### RTS Threshold

Description | The Request To Send (RTS) threshold is the size at which the Access Point will issue a Request to Send frame before sending the packet.
Valid Range | 256 - 2346.

### Max RTS Retries

Description | The maximum number of times the Access Point will issue a Request to Send frame before stopping the attempt to send the packet from the radio.
Valid Range | 1 - 128

### Max Data Retries

Description | The maximum number of attempts to send a packet before giving up and dropping a packet.
Valid Range | 1 - 128

### Beacon Interval

Description | The amount of time in Time Units (TU) between beacons. One TU is 1024 microseconds.
Valid Range | 20 - 1000

### DTIM Interval

Description | The DTIM (Delivery Traffic Information Message) interval in beacon intervals.
Valid Range | 1 - 16384

### Restart AP

Description | Button for restarting the Access Point. When Restart AP is pressed, the Access Point requests user confirmation.

### Apply

Description | Button for applying new settings. Most settings become effective only after the Access Point is restarted. When Apply is pressed, the Access Point requests user confirmation.

## Radio 802.11b

### BSSID

Description | The BSSID (Basic Service Set Identifier) of the radio 802.11b.
Valid Range | MAC address of the form nn:nn:nn:nn:nn:nn

### Authentication Type

Description | The type of authentication algorithm required to be used by a client station attempting to authenticate with the Access Point. "Shared" authentication requires the Access Point and stations to use the authentication key indicated by the "Default WEP Key" setting on the "WEP Settings 802.11b" page. That key must be defined in order for “Shared” to be used.
Valid Range | Open, Shared.
Default | Open.

### SSID

Description | Service Set Identifier String. The Access Point broadcasts this string in its beacons.
Valid Range | 1 - 32 characters
Default | 101

### Radio Channel

Description | The frequency at which the radio operates.
Valid Range | 1 [2,412 GHz], 2 [2.417 GHz], 3 [2.422 GHz], 4 [2.427 GHz], 5 [2.432 GHz], 6 [2.437 GHz], 7 [2.442 GHz], 8 [2.447 GHz]. 9 [2.452 GHz], 10 [2.457 GHz], 11 [2.462 GHz]

### Transmit Power

Description | The radio transmission power level.
Valid Range | 1mW, 5mW, 15mW, 30mW

### Fragment Threshold

Description | The Fragmentation threshold is the size at which packets will be fragmented and transmitted piecemeal instead of all at once.
Valid Range | 256 - 2338

### RTS Threshold

Description | The Request To Send (RTS) threshold is the size at which the Access Point will issue a Request to Send frame before sending the packet.
Valid Range | 0 - 2339

### Max RTS Retries

Description | The maximum number of times the Access Point will issue a Request to Send frame before stopping the attempt to send the packet from the radio.
Valid Range | 1 - 128

### Max Data Retries

Description | The maximum number of attempts to send a packet before giving up and dropping a packet.
Valid Range | 1 - 128

### Beacon Interval

Description | The amount of time in Time Units (TU) between beacons. One TU is 1024 microseconds.
Valid Range | 1 - 65535

### DTIM Interval

Description | The DTIM (Delivery Traffic Information Message) interval in beacon intervals.
Valid Range | 1 - 255

### Restart AP

Description | Button for restarting the Access Point. When Restart AP is pressed, the Access Point requests user confirmation.

### Apply

Description | Button for applying new settings. Most settings become effective only after the Access Point is restarted. When Apply is pressed, the Access Point requests user confirmation.

## Ethernet Setup

### Current IP Address

Description | The IP address currently used by the Access Point. If DHCP is enabled and available, this is the address assigned dynamically by the DHCP server, otherwise this is Default IP Address .
Valid Range | Valid IP address format.

### Current Subnet Mask

Description | The subnet mask currently used by the Access Point. If DHCP is enabled and available, that address is assigned dynamically by the DHCP server. Otherwise the Default Subnet Mask is used.
Valid Range | Valid IP address format.

### Current Speed

Description | The speed and duplex mode the Ethernet is currently using. This will be the negotiated result when the setting is “Auto”, or it will be the specified Speed setting.
Valid Range | 10BaseTHalfDuplex, 100BaseTHalfDuplex, 10BaseTFullDuplex, 100BaseTFullDuplex.

### Speed

Description | The speed and duplex mode of the Ethernet interface. Normally “Auto” is used and is the recommended setting because with this setting, the Ethernet device will negotiate a setting depending on the link it is connected to. Using settings other than “Auto” forces the Ethernet device to that setting (no negotiation) which may not work depending on the link it is connected to.
Valid Range | Auto, 10BaseTHalfDuplex, 100BaseTHalfDuplex, 10BaseTFullDuplex, 100BaseTFullDuplex.
Default | Auto

## Radio Statistics 802.11a/802.11b

### MAC Address

Description | The MAC address of the Access Point.
Valid Range | MAC address of the form nn:nn:nn:nn:nn:nn

### Transmit Statistics, Unicast Packets

Description | The number of unicast packets transmitted to client stations.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Multicast Packets

Description | The number of multicast packets transmitted to client stations.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Wrong Packets

Description | The number of packets presenting errors received from the Ethernet device. A non-zero count may indicate a failure of the Ethernet device.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Max Retry Packets

Description | The number of packets that could not be transmitted after being retried the maximum number of times.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Total Retries

Description | The number of packets for which the radio retried the transmission.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Management Packets

Description | The number of management packets sent to client stations.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Beacons

Description | The number of beacon packets broadcast by the Access Point radio.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Data Retries

Description | The number of data packets whose transmission to client stations had to be retried by the Access Point radio.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Single Collision Pkts OK

Description | The number of packets whose transmission was retried once because of a collision error.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Multiple Collision Pkts OK

Description | The number of packets whose transmission was retried more than once because of collision errors.
Valid Range | Positive integer (0 included).

### Transmit Statistics, Ack Failed

Description | The number of packets sent to client stations for which the Access Point radio did not receive the expected ACK.
Valid Range | Positive integer (0 included).

### Receive Statistics, Unicast Packets

Description | The number of unicast packets received from client stations.
Valid Range | Positive integer (0 included).

### Receive Statistics, Multicast Packets

Description | The number of multicast packets received from client stations.
Valid Range | Positive integer (0 included).

### Receive Statistics, Wrong Packets

Description | Total packets received from client stations presenting errors.
Valid Range | Positive integer (0 included).

### Receive Statistics, CRC Errors

Description | The number of packets with CRC errors received from client stations.
Valid Range | Positive integer (0 included).

### Receive Statistics, WEP Errors

Description | The number of packets with WEP errors received from client stations.
Valid Range | Positive integer (0 included).

### Receive Statistics, Overrun Packets

Description | The number of packets received from client stations that were discarded because the Access Point had a temporary overload of packets to handle.
Valid Range | Positive integer (0 included).

### Receive Statistics, Duplicate Packets

Description | The number of packets from client stations that were received twice because a lost acknowledgment with a retransmit from the sender.
Valid Range | Positive integer (0 included).

### Receive Statistics, Life Exceeded Packets

Description | The number of fragmented data packets received from client stations that were dropped because it took too long to get the next fragment.
Valid Range | Positive integer (0 included).

### Receive Statistics, Management Packets

Description | The number of management packets received from client stations.
Valid Range | Positive integer (0 included).

### Receive Statistics, Beacons

Description | The number of beacons received from client stations. This counter should stay 0 for proper operation of client stations in an infrastructure wireless LAN.
Valid Range | Positive integer (0 included).

### Receive Statistics, PLCP CRC Errors

Description | The number of packets received from client stations presenting CRC errors in the PLCP header.
Valid Range | Positive integer (0 included).

### Clear Statistics

Description | Button to clear Ethernet statistics.

### Refresh Statistics

Description | Button to refresh Ethernet statistics.

## SNMP Agent

### Trap Destination

Description | The IP address of the server running SNMP management software.
Valid Range | 0 - 255 characters

### Trap Community

Description | SNMP community name.
Valid Range | 0 - 255 characters

### Read Community

Description | Password that allows the user to perform SNMP "get" commands.
Valid Range | 0 - 32 characters

### Write Community

Description | Password that allows the user to perform SNMP "set" commands.
Valid Range | 0 - 32 characters

### AP Location

Description | Text indicating the Access Point location.
Valid Range | 0 - 32 characters

### System Contact

Description | The name of the technician responsible for Access Point maintenance.
Valid Range | 0 - 32 characters
Default | Empty string.

### Restart AP

Description | Button for restarting the Access Point. When Restart AP is pressed, the Access Point requests user confirmation.

### Apply

Description | Button for applying new settings. Most settings become effective only after the Access Point is restarted. When Apply is pressed, the Access Point requests user confirmation.

## SNTP Server

Description | The IP address of the SNTP (Simple Network Time Protocol) server.
Valid Range | 0 - 255 characters

### Restart AP

Description | Button for restarting the Access Point. When Restart AP is pressed, the Access Point requests user confirmation.

### Apply

Description | Button for applying new settings. Most settings become effective only after the Access Point is restarted. When Apply is pressed, the Access Point requests user confirmation.

## Change Login Info

### User Name

Description | The name to be provided by the user in order to gain access to the Access Point management pages.
Valid Range | 1 - 32 characters

### Password

Description | The new password to be provided by the user in order to gain access to the Access Point management pages.
Valid Range | 5 - 12 characters, except colon ":".

### Confirm Password

Description | The new password needed to be provided by the user in order to gain access to the Access Point management pages. Should be identical with the content of the "Password" field.
Valid Range | 5 - 12 characters, except colon ":"

### Apply

Description | Button for applying new settings. Most settings become effective only after the Access Point is restarted. When Apply is pressed, the Access Point requests user confirmation.

## WEP Settings 802.11a/802.11b

### WEP (Wired Equivalent Privacy)

Description | The usage of the WEP keys.
Valid Range | Enabled, Disabled.
Default | Disabled.

### Default WEP Key

Description | The index of the default WEP key.
Valid Range | 1 ... 4

### WEP Key

Description | The WEP key string.
Valid Range | 10 hex digits for 64-bit encryption, or 26 hex digits for 128-bit encryption. A hex digit is a character in the following range: '0'... '9', 'A'... 'F', 'a'... 'f'.

### Restart AP

Description | Button for restarting the Access Point. When Restart AP is pressed, the Access Point requests user confirmation.

### Apply

Description | Button for applying new settings. Most settings become effective only after the Access Point is restarted. When Apply is pressed, the Access Point requests user confirmation.

### WEP Key Storage and Display

A WEP key is subject to the following rules:

- Once set, a WEP key cannot be deleted, but it can be overwritten
- The WEP key is only displayed when it is being set

The presence or absence of a WEP key is indicated by the read-only status field on the right side of the WEP key field:

- None: key not set
- 64 bit: a 64-bit encryption key has been set
- 128 bit: a 128-bit encryption key has been set

- Copyright © 2002 Intel Corporation. Legal Information