# Intel PRO/1000 Gigabit Adapter Specifications**

Product Feature | PRO/1000 Gigabit Server Adapter | PRO/1000 F Server Adapter | PRO/1000 T Server Adapter | PRO/1000 T Desktop Adapter | PRO/1000 XT Server Adapter | PRO/1000 XF Server Adapter
--- | --- | --- | --- | --- | --- | ---
Bus Connector* | PCI 2.1 (33 Mhz only) | PCI 2.2 | PCI 2.2 | PCI 2.2 (33/66 Mhz, 32-bit only) | PCI 2.2 PCI-X 1.0a | PCI 2.2 PCI-X 1.0a
Transmission Mode/Connector | SX/Optical Fiber | SX/Optical Fiber | Twisted copper/ RJ-45 | Twisted copper/ RJ-45 | Twisted copper/ RJ-45 | SX/Optical Fiber
Cabling | 1000Base-SX | 1000Base-SX | 1000Base-T (CAT5) | 1000Base-T (CAT5) | 1000Base-T (CAT5) | 1000Base-SX
Power requirements | Power support provided for both 5.0 v and 3.3v aux. with key form factor for both signaling voltages
1.0A @ +5VDC (5.0 Watts) | 1.0A @ +5VDC (5.0 Watts) | 1.18A @ +5VDC (5.9 Watts) | 1.25A @ +5VDC (6.25 Watts) | 1.25A @ +5VDC (6.25 Watts) | 0.9A @ +5VDC (4.48 Watts)
Interrupt | INTA | INTA | INTA | INTA | INTA | INTA
Dimensions (excluding bracket) | 6.42 x 3.25 in. 16.31 x 8.26 cm | 6.42 x 3.25 in. 16.31 x 8.26 cm | 6.42 x 3.40 in. 16.31 x 8.64 cm | 4.70 x 2.00 in. 11.94 x 5.08 cm | 6.39 x 2.53 in. 16.22 x 6.42 cm | 6.39 x 2.50 in. 16.22 x 6.35 cm
Weight | 2.82 oz. 80 grams | 2.82 oz. 80 grams | 3.36 oz. 95.3 grams | 3.36 oz. 95.3 g. | 3.36 oz. 95.3 grams | 3.36 oz. 95.3 grams
Temperature | All Adapters: Operating: 32 - 131° F, 0 - 55° C; Non-operating: -40 to +70° C
MTBF | 22 years | 22 years | 106 years | 135 years | 135 years | 126 years
Available Speeds | 1000 only | 1000 only | 10/100/1000 auto-negotiate | 10/100/1000 auto-negotiate | 10/100/1000 auto-negotiate | 1000 only
Duplex modes | Full only | Full only | Full or half at 10/100 Mbps; full only at 1000 Mbps. | Full or half at 10/100 Mbps; full only at 1000 Mbps. | Full or half at 10/100 Mbps; full only at 1000 Mbps. | Full only
Standards conformance | IEEE 802.1p IEEE 802.3ac IEEE 802.3ad IEEE 802.3x IEEE 802.3z PCI 2.1 | IEEE 802.1p IEEE 802.1Q IEEE 802.3ac IEEE 802.3ad IEEE 802.3u IEEE 802.3x IEEE 802.3z PCI 2.2 | IEEE 802.1p IEEE 802.1Q IEEE 802.3ab IEEE 802.3ac IEEE 802.3ad IEEE 802.3u IEEE 802.3x PCI 2.2 ACPI v1.0 | IEEE 802.1p IEEE 802.1Q IEEE 802.3ab IEEE 802.3ac IEEE 802.3u IEEE 802.3x PCI v2.2 ACPI v1.0 | IEEE 802.1p IEEE 802.1Q IEEE 802.3ab IEEE 802.3ac IEEE 802.3ad IEEE 802.3u IEEE 802.3x PCI v2.2 ACPI v1.0 PCI-X v1.0 | IEEE 802.1p IEEE 802.1Q IEEE 802.3ac IEEE 802.3ad IEEE 802.3x IEEE 802.3z PCI 2.2 ACPI v1.0 PCI-X v1.0
Indicator Lights single color dual color | TX Activity RX Activity Link Identity | TX Activity RX Activity Link Identity | Link Rx/Tx Activity Speed Identity/Bus ID | Link & Activity/ Identity Speed | Link & Activity/Identity Speed | Link Activity [Identity]
Regulatory and Safety | All adapters: FCC Class B Radiated and Conducted Emissions requirements for U.S. and Canada VCCI Class B Radiated and Conducted Emissions requirements for Japan BSMI Class B Radiated and Conducted Emissions requirements for Taiwan CISPR 22 Class B Radiated and Conducted Emissions requirements for Australia/New Zealand EN55022 Class B Radiated and Conducted Emissions requirements for European Union (EU) EN55024 Immunity requirements for European Union (EU) EN60950 Safety requirements for European Union (EU) UL (Underwriter’s Laboratories) and Canada UL Safety requirements

Also see: How to Identify your Adapter

More adapter information is at the Intel Support web site.

**Intel adapter feature support may be limited by the hardware, OS and driver software for your particular platform.

## Standards

- IEEE 802.1p: Priority Queuing (traffic prioritizing) and Quality of Service levels
- IEEE 802.1Q: Virtual LAN identification
- IEEE 802.3ab: Gigabit Ethernet over copper
- IEEE 802.3ac: Tagging
- IEEE 802.3ad: Link Aggregation (static mode is supported on indicated Intel adapters)
- IEEE 802.3u: Fast Ethernet
- IEEE 802.3x: Flow Control
- IEEE 802.3z: Gigabit Ethernet over optical fiber
- ACPI: Advanced Configuration and Power Management
- PCI: system bus specification: 32/64-bit, 33/66 Mhz (any combination, unless otherwise noted)
- PCI-X: system bus specification: 64-bit, 66/100/133 Mhz (any combination)

More information on IEEE 802 standards available at http://www.ieee802.org.

IEEE 802.3ac VLANs:

VLANs require VLAN capable switches either implicit (switch only) or explicit (IEEE 802.3ac). IEEE 802.3ac VLANs allow multiple VLANs per adapter or team since both the switch and adapter use a tag in the packet header to sort VLANs.

All PRO/1000 server adapters fully support IEEE 802.3ac VLANs when attached to an explicit VLAN enabled switch.

## Cabling

- 1000Base-SX on 850 nanometer optical fiber:

  - Utilizing 50 micron multimode, length is 550 meters max.

  - Utilizing 62.5 micron multimode, length is 260 meters max.

- 1000BaseT on Category 4, or Category 5 wiring, twisted 4-pair copper.

  - Length is 100 meters max.

  - Category 3 wiring supports only 10Mbps.

## Ethernet MAC Addresses

### Single-Port Adapters

The Ethernet address is printed on the identification sticker on the front of the card.

### Dual-Port Adapters

There are two types of dual port adapters: a 32-bit adapter with part numbers 715191-00x or 751110-00x, and a 32/64-bit adapter with part numbers A28276-00x. On both types, the adapter's 12-digit, hexadecimal Ethernet address is printed on a sticker placed on the adapter, or can be found in the system's BIOS setup. The Ethernet address is sometimes called the node address or the MAC address.

For 32-bit dual port adapters, the Ethernet address printed on the identification sticker refers to the port closest to the PCI slot. Add 1 to the printed address to find the address of the 2nd port. For example, if the Ethernet address on the sticker reads xxxxxxxxxx77, then the address of the 2nd port (the one farthest from the slot) would be xxxxxxxxxx78.

For 32/64-bit dual port adapters, the Ethernet address printed on the identification sticker refers to the port farthest from the slot. Add 1 to the printed address to find the address of the 2nd port. For example, if the Ethernet address on the sticker reads xxxxxxxxxx77, then the address of the 2nd port (the one closest to the PCI slot) would be xxxxxxxxxx78.

### Integrated Adapters

On a system with the LAN integrated on the motherboard, the identification sticker is usually located on the motherboard near the network connector.

Copyright © 2002 Intel Corporation. Legal Information