## Forwarding Counts

Forwarding Counts provides information on packets transmitted from one interface to another (Ethernet, RF, AP). Forwarding Counts also displays the broadcast packets transmitted from the Intel® PRO/Wireless 2011B LAN Access Point.

### Web Interface

1. Select Forwarding Counts from the Statistics Menu at the left side of the screen.
2. Click Start Refresh to update the values on the screen.
3. When finished, click Stop Refresh.

### Management Console

1. Select Forwarding Counts from the Main Menu .
2. Select Refresh at the status display to update the values manually.
3. Select Timed to automatically update the display every two seconds.
4. Press ESC to return to the previous menu.

Copyright© 2002 Intel Corporation. Legal Information