## Wireless Network Topologies

#### Basic Network Configurations

You can use Intel® PRO/Wireless LAN Access Points in any of several network configurations depending on your networking needs and size. The following examples illustrate some simple wireless network configurations with access points:

- A single access point forms a single-cell wireless network.

- A single access point can bridge between the Ethernet and wireless networks.

- Multiple access points can coexist as separate, individual networks at the same site using different network names (SSID). These separate wireless LANs can be configured to use different channel assignments to avoid RF interference.

- Multiple access points wired together provide a network with a better coverage area and performance when using the same Network Names (SSIDs).

#### Wireless LAN Access Point (WLAP) Mode

The following illustrations show possible options for access points operating in WLAP mode. In WLAP mode, an access point forwards data to another access point using the wireless connection rather than Ethernet cabling.

- Access points can bridge between two Ethernet networks.

- An access point can operate as a repeater to extend coverage area without additional network cabling.

- Multiple access points can form a standalone wireless network. Each access point can connect with up to four other access points.

Copyright© 2002 Intel Corporation. Legal Information