            SiS 900/7016 PCI Fast Ethernet Adapter Installation
              ODI Driver for Client32 in DOS/Windows 3.x

(1) Install Driver While setting up your Client32:
컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴

    1. When the Installation program ask you to "Select a LAN Driver Type",
       select "32-bit LAN Drivers".

    2. In "32-Bit Network Board Drivers" window, select "USER SPECIFIED 32
       BIT DRIVER".

    3. Insert the driver diskette into your floppy drive, and specify the
       path of the driver in the diskette(i.e. A:\CLIENT32\) to copy
       the driver files to your system.

    4. Select "SiS 900/7016 PCI Adapters Netware ODI32 Driver".

    5. Press <F10> to finish the Settings for SiS PCI....

    6. Press <F10> to save installation configuration.

    7. Press <Ctrl><Alt><Del> to restart the system.

    Note: A STARTNET.BAT file will be generated in the Client32 directory.
          (ex. C:\NOVELL\CLIENT32 )


(2) System with existing Netware client32 programs:
컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴

    1. Copy the LAN driver and LDI file to the Client32 directory.
       ex. C:\Novell\client32

    2. Edit your STARTNET.BAT file in your Client32 directory. Add the
       following:

       LOAD C:\NOVELL\CLIENT32\SIS900.LAN FRAME=Ethernet_802.2

    3. Execute STARTNET.BAT to connect to Server.

    Note: Content of STARTNET.BAT (for 32-bit LAN driver)

       SET NWLANGUAGE=ENGLISH
       C:\NOVELL\CLIENT32\NIOS.EXE
       LOAD C:\NOVELL\CLIENT32\LSLC32.NLM
       LOAD C:\NOVELL\CLIENT32\CMSM.NLM
       LOAD C:\NOVELL\CLIENT32\ETHERTSM.NLM
       LOAD C:\NOVELL\CLIENT32\SIS900.LAN FRAME=Ethernet_802.2
       LOAD C:\NOVELL\CLIENT32\SIS900.LAN FRAME=Ethernet_802.3
       LOAD C:\NOVELL\CLIENT32\IPX.NLM
       LOAD C:\NOVELL\CLIENT32\CLIENT32.NLM
