### 3A

1:1

1:n

No. | Name | Note
--- | --- | ---
(1) | COM port conversion adapter by Pro-face CA3-ADPCOM-01 |
(2) | Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 |
(3) | Cable by YASKAWA CONTROLS CO., LTD FADHOWA-50 (0.5m) |

NOTE

- Example of cable image
  In the example above, the cable color is orange, and the identification mark shows red dot-line, which means TXD.
- Cable length: 30m or less.