### MP3000 Series / Sub CPU

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
System registers | SB000000 - SB65534F | SW00000 - SW65534 |  |
Input registers | IB000000 - IB27FFFF | IW00000 - IW27FFF | *1
Output registers | OB000000 - OB27FFFF | OW00000 - OW27FFF | *1
Data registers | MB00000000 - MB1048575F | MW0000000 - MW1048575 |
G registers | GB000000000 - GB02097151F | GW00000000 - GW02097151 |

*1As for Input and Output registers, device 0x9000-0xFFFF cannot be written.

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms