### 3H

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (plug) External Device side: Accessory box | Instead of connecting the Display (FG), connect the Shield to the Shell.

IMPORTANT:

- The 5V output (Pin #6) on the Display is the power for the Siemens AG's PROFIBUS connector. Do not use it for other devices.

NOTE

- The cable length have to be 10m or less.
  Max length between the Display and the "Accessory Box connected to Display". Total cable length between accessory boxes have to be 1000m or less.