### 3B

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (socket) External Device side: Accessory box | Instead of connecting the Display (FG), connect the Shield to the Shell.

NOTE

- The cable length have to be 10m or less.
  Max length between the Display and the "Accessory Box connected to Display". Total cable length between accessory boxes have to be 1000m or less.