### 3G

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block External Device side: Accessory box |

NOTE

- The cable length have to be 10m or less.
  Max length between the Display and the "Accessory Box connected to Display". Total cable length between accessory boxes have to be 1000m or less.

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | ON