### 3B

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (socket) SIO converter side: D-Sub 9 pin (socket) |
(2) | SIO converter by IAI Corporation RC*-TU-SIO-* |
(3) | User-created cable Connector SIO converter side (J4 or J5): e-CON connector (plug) Junction side: e-CON connector (plug) |
(4) | Junction by AMP 5-1473574-4 |
(5) | Controller link cable by IAI Corporation CB-RCB-CTL002 |
(6) | Termination resistance Connector Junction side: e-CON connector (plug) |
(7) | User-created cable Connector Junction side: e-CON connector (plug) |

NOTE

- Cable length from Display to SIO converter: 15m or less
- Cable length from SIO converter to External Device: 100m or less