### 2H

1:1

1:n

No. | Name | Note
--- | --- | ---
(1) | User-created cable Connector Display side: D-sub 9 pin (plug) External Device side: Terminal Block |

IMPORTANT

- The 5V output (Pin #6) on the Display is the power for the Siemens AG’s PROFIBUS connector. Do not use it for other devices.

NOTE

- For the shield ground, be sure to use the ground terminal on the External Device.
- Turn on the termination resistor switch on the External Device located at the end.
- Cable length: 50m or less.