### External Device Settings

Use the ladder software "PL7 PRO" for communication settings.

For setting, go to "Configuration" in "Application Browser" of "PL7 PRO", "Hardware Configuration", and "ETY PORT" in this order.

Setup Items | Setup Description
IP address configuration | Configured (Fixed)
IP address | Optional
Ethernet configuration | Ethernet II (Fixed)

##### Notes

- Check with the network administrator about the IP address. Do not duplicate IP addresses.

- Please refer to the manual of the ladder software for details on other settings.

- Use an integer from 0 to 255 to enter the unit ID of the External Device.