### 7G

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block RS232C conversion unit side: D-Sub 9 pin (plug) |
(2) | RS232C conversion unit by IAI Corporation RCB-CV-MW |
(3) | Communication cable by IAI Corporation CB-RCA-SIO050 |
(4) | SIO converter by IAI Corporation RC*-TU-SIO-* |
(5) | User-created cable Connector SIO converter side TB1: Link connection terminal block TB2: Power supply and emergency stop terminal block Power & I/O Cable side: Terminal block |
(6) | Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB |

NOTE

- When connecting to more than one equipment, connect the terminal block.
- Cable length from SIO converter to External Device: 100m or less

*1 We recommend the IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB as the Power & I/O Cable.