### 1B

No. | Name | Note
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block External Device side: D-sub 9 pin (plug) |
(2) | Loader connecting cable by Fuji Electric Systems Co., Ltd. PXH or PUM Connector Display side: D-sub 9 pin External Device side: φ2.5 triple pole miniature jack |

NOTE

- Connect the loader connecting cable to the PC loader port of the External Device.