### 6I)

Legend | Name | Note
--- | --- | ---
(1) | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 |
(2) | User-created cable Connector Display side: Terminal block External Device side: Terminal block. |

NOTE

- Termination resistance of 120Ω is built into the External Device.
- For the External Device connector, use the XA connector (XAP-03V-1) by J.S.T. Mfg.
- Cable length: 500m or less.