### 3A)

No. | Name | Notes
--- | --- | ---
(1) | COM Port Conversion Adapter by Pro-face CA3-ADPCOM-01 |
(2) | Terminal Block Conversion Adapter by Pro-face CA3-ADPTRM-01 |
(3) | User-created cable Connector Display side: Terminal block External Device side: MR-8 (plug) |

NOTE

- When the External Device has the SG terminal, connect it to the SG terminal of the Display.
- Cable length: 300m or less.