### 5I

No. | Name | Notes
--- | --- | ---
(1) | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 |
(2) | User-created cable Connector Display side: Terminal block External Device side: Uni-Telway cable | Instead of connecting the Display (FG), connect the Shield to the Shell.
(3) | Uni-Telway cable by Schneider Electric Industries TSX SCP CU 4030 (3m) |
(4) | PCMCIA card for RS485 by Schneider Electric Industries TSX SCP 114 |