### External Device Settings

Use the ladder software "PL7 PRO" for communication settings.

Execute "Hardware Configuration" from "Configuration" in "Application Browser" of "PL7 PRO" to display the "Configuration" dialog box. Double-click the empty slot to display the "Add Module" dialog box. Select "Communication" in the "Family" field. Then select "Link Unit" display in the "Module" field to display the screen for setting.

Setup Items | Setup Description
IP address configuration | Configured (Fixed)
IP address | Optional
Ethernet configuration | Ethernet II (Fixed)

##### Notes

- Check with the network administrator about the IP address. Do not duplicate IP addresses.

- Please refer to the manual of the ladder software for details on other settings.

- Use an integer from 0 to 255 to enter the unit ID of the External Device.