### 5A

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | COM port conversion adapter by Pro-face CA3-ADPCOM-01 |
(2) | Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 |
(3) | User-created cable Connector Display side: Terminal block Power & I/O Cable side: Terminal block |
(4) | Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB |

NOTE

- Cable length: 100m or less

*1 We recommend the IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB as the Power & I/O Cable.