### 2B)

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (socket) External Device side: RS485 port |

NOTE

- The cable length is normally 1000m or less, depending on the External Device. Refer to your External Device manual for details.
- The connection method and termination resistance depends on the External Device.
- The termination resistance on the Display is not isolated.