### Supported Device

Device | Bit Address | Word Address | 32bits | Notes
--- | --- | --- | --- | ---
Input Points | %IX0.0.0 - %IX9.7.63 | %IW0.0.0 - %IW9.7.3 |  | *1
Output Points | %QX0.0.0 - %QX9.7.63 | %QW0.0.0 - %QW9.7.3 | *1
Data Memory | %MX000000 - %MX524287 | %MW00000 - %MW32767 |

*1Device explanation:

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms