Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) STM6000 (COM1) PC/AT IPC*2 | 12A | RS-232C Cable by Mitsubishi Electric F2-232CAB-1 (3m) + RS232C/RS422 Signal Converter by Mitsubishi Electric FX-232AWC or FX-232AW + RS-422 Cable by Mitsubishi Electric FX-422CAB0 (1.5m) |

*2Only the COM port which can communicate by RS-232C can be used.

IPC COM Port