### 5I

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 |
(2) | User-created cable Connector Display side: Terminal block Power & I/O Cable side: Terminal block |
(3) | Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB |

NOTE

- Cable length: 100m or less

*1 We recommend the IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB as the Power & I/O Cable.