### 6A)

Legend | Name | Note
--- | --- | ---
(1) | COM port conversion adapter by Pro-face CA3-ADPCOM-01 |
(2) | Connector terminal block conversion adapter by Pro-face CA3-ADPTRM-01 |
(3) | User-created cable Connector Display side: Terminal block External Device side: Terminal block |

NOTE

- Termination resistance of 120Ω is built into the External Device.
- For the External Device connector, use the XA connector (XAP-03V-1) by J.S.T. Mfg.
- Cable length: 500m or less.