### Settings of External Device

External Device settings vary depending on the device. Refer to your External Device manual for details.

##### Setup items

Setup items | Setting
--- | ---
Connection Format | RS-232C
Baud Rate | 19200 bps
Parity Bit | Even
Stop Bit | 1 bit
Tx Wait Time | 2 ms
Mode/Data Bits | RTU (8)
Station Address | 1

NOTE

- Use an integer from 1 to 247 to enter the unit ID of the External Device.