### Inverter Series

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
Bit registers*1 | BR0000.0 - BR195C.F | - | - | *2
Registers*1 | - | 0000~195C |  | *2

*1In the Inverter, bit registers and registers use the same device. Bit registers are used only for bit addresses.
The access method when specifying bits varies depending on the device.

Bit registers BR0000.0 - BR195C.F

Registers

*2The available register numbers and available read/write operations differ depending on the External Device model. For further information, refer to the instruction manual for your External Device.

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms