### 2H)

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | RS-422 terminal block conversion adapter by Pro-face PFXZCBADTM1 |
(2) | User-created cable Connector Display side: Terminal block External Device side: Depends on the specification of the External Device.

NOTE

- When the RDB terminal of PFXZCBADTM1 to the TRM terminal, the termination resistance of 100Ω (1/2W) is inserted between RDA and RDB terminals on the Display.
- Cable length: 1000m or less.