### Settings of External Device (LMC x00C unit)

Use the EcoStruxure Machine Expert software for the External Device to define its communication settings. Please refer to the External Device manual for more details.

1. Start EcoStruxure Machine Expert and create a new project.

2. Select "EcoStruxure Machine Expert" from the [Controller] pull-down menu.

3. Double click on the Device (PacDrive LMC x00C) in the device window at the left screen edge.

4. Right-click the controller in the tab Controller selection of the device window.

5. Select [Edit communication settings] in the context menu.
   Check [IP address], [Subnet mask] and [Gateway].

NOTE

- When the External Device uses the UserManagement function, input the login information in “Username” and “Password” under the driver property of BLUE or hardware configuration for Display.

- When using the encrypted communication, select the "Encrypted communication" check box in either the driver's equipment properties in BLUE, or in the Hardware Configuration.