### 1F

1:1

1:n

No. | Name | Note
--- | --- | ---
(1) | RS-422 terminal block conversion adapter by Pro-face PFXZCBADTM1 |
(2) | User-created cable Connector Display side: Terminal Block External Device side: Terminal Block |

NOTE

- For the shield ground, be sure to use the ground terminal on the External Device.
- Turn on the termination resistor switch on the External Device located at the end.
- Cable length: 50m or less.