# Properties (USB Barcode Reader)

You can configure the details of the USB barcode reader in System Architecture.

1. In the Project Explorer window, go to [System Architecture] and click [Accessories].

2. On the System Architecture editor toolbar, click [USB Barcode Reader].

3. In the Properties window, configure the properties below.

## Basic

[Save Data In]

You can set up the following destinations for data entered from a USB barcode reader. Select [Objects] or [Variable].

[Scanned String]

You can set up internal STRING variables for data entered from a USB barcode reader. Setup is possible only when [Variable] is selected in [Save Data In].

[Scanned String (bytes)]

To count the characters, set up an internal integer variable as the save destination for the counted value. Setup is possible only when [Variable] is selected in [Save Data In].

[Key Code]

Select the keyboard layout. Select [English 101] or [Japanese 106].