# Properties (Recipe Control)

[Recipe Family ID] 'RecipeControl1.FamilyID'
Set the recipe family ID to use.
Note: You can also change the recipe family ID with the Recipe Dropdown List. Data Binding Support: To use as a Binding Source, refer to the following. RecipeControl1.FamilyID When used as a Binding Target, the Binding Sources that can be associated are as follows. [ Alarm] [ Variable] [ Target] [ Equipment] [ Recipe] For more information of Data Binding concept, refer to the following. Data Binding

[Recipe Group ID] 'RecipeControl1.GroupID'
Set the recipe group ID to use.
Note: You can also use a Recipe Dropdown List to change the recipe group ID. Data Binding Support: To use as a Binding Source, refer to the following. RecipeControl1.GroupID When used as a Binding Target, the Binding Sources that can be associated are as follows. [ Alarm] [ Variable] [ Target] [ Equipment] [ Recipe] For more information of Data Binding concept, refer to the following. Data Binding

[Recipe ID] 'RecipeControl1.RecipeID'
Set the recipe ID to use.
Note: You can also use a Recipe Dropdown List to change the recipe ID. Data Binding Support: To use as a Binding Source, refer to the following. RecipeControl1.RecipeID When used as a Binding Target, the Binding Sources that can be associated are as follows. [ Alarm] [ Variable] [ Target] [ Equipment] [ Recipe] For more information of Data Binding concept, refer to the following. Data Binding

[Export/Import Data Location]
Select the export/import location of recipe data. -[Local Storage] -[SD Card] -[USB Storage]
Note: The storage which can be selected for [Export/Import Data Location] depends on the display unit model. When using SP5000 Series Open Box (Windows 10 IoT Enterprise Model), IPC Series, or PC/AT, simply selecting [SD Card] or [USB Storage] will NOT store the export file in the SD card or USB storage inserted in the display unit. To save the export file in the SD card or USB storage, specify the destination folder in the [Destination Folder (SD Card)] or [Destination Folder (USB Storage)] property of the target. [Target01] property window > [Function] tab > [Options] tab > [Preferences] Properties (Target01)

[Folder Name]
Set the name of the folder where the exported file is saved. (Example: \Recipe) You can use a maximum 256 characters, excluding the following symbols, for the folder name. : ; | , * ? " < >
Note: On the IPC Series, to use a specific language for folder and file names, set up in [Control Panel] > [Change system locale].

[Recipe Data Direction]
Select the direction of exported data. -[Ingredient_Recipe]: Each line in the exported file is a recipe. Ingredients are in columns. -[Recipe_Ingredient]: Each line in the exported file is an ingredient value. Recipes are in columns. This setting applies to exports from both the screen editing software and display unit.

[Save in]
Select the location of recipe data from the following. -[Internal] (application memory) -[SD Card] -[USB Storage]
Important: When you use external storage for saving recipe data, turn off the display unit before removing the external storage. If you remove external storage before turning off the display unit, the recipe data cannot save even though the external storage is inserted again. In this scenario, restart the display unit after inserting external storage. We recommend you avoid selecting external storage that is often removed from the display unit. Note: The memory and storage which can be selected for [Save in] depend on the display unit model. When using SP5000 Series Open Box (Windows 10 IoT Enterprise Model), IPC Series, or PC/AT, simply selecting [SD Card] or [USB Storage] will NOT store the recipe data in the SD card or USB storage inserted in the display unit. To save the recipe data in the SD card or USB storage, specify the destination folder in the [Destination Folder (SD Card)] or [Destination Folder (USB Storage)] property of the target. [Target01] property window > [Function] tab > [Options] tab > [Preferences] Properties (Target01) For information on application memory, refer to the following. Functions Available in Memory / Storage

[Encryption]
Select this check box to encrypt the recipe data. This property is available when external storage is selected in [Save in]. The default value is enabled. Clear this check box if you do not want to encrypt the recipe data.