# Properties (System String Keypad)

[Key Label]
Set the label of the displayed key.
When used as a Binding Target, the Binding Sources that can be associated are as follows. [ Language Table Text] For more information of Data Binding concept, refer to the following. Data Binding

[Font Type]
Select the desired language for the characters used on the keypad.

[Keyboard touch detection]
Select the timing for when the keypad touch is detected.
[Click] Touch the key then release, at which point the touch is detected. : Detect touch Press: Key is pressed Release: Key is not pressed Note: While the key is pressed and without releasing, if you move your finger outside the area of the key, the touch is canceled. While the key is pressed and any of the following occurs, the touch is canceled. Object does not display anymore due to a screen or content change. The interlock function is enabled on the object. The user logs out. Project file is transferred. Run time is shutdown. Run time is restarted. The Windows active window changes from the run-time application to a different application. [Press] Touch the key, at which point the touch is detected. : Detect touch Press: Key is pressed Release: Key is not pressed

[Keypad Width]
Select the [Set Keypad Width] check box to specify the width (768...3840) of the [System String Keypad]. The keypad height is adjusted with respect to the keypad width.
Note: If you set a keypad width greater than the screen width, during operation the keypad width is adjusted to fit the screen width.