Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) ST6000 2nd Gen*d-4 (COM1) STM6000 (COM1) PC/AT IPC*2 | 8A | RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable for PC connection by IAI Corporation CB-ERC2-SIO020 + Power & I/O Cable by IAI Corporation CB-ERC2-PWBIO*** or CB-ERC2-PWBIO***-RB |
GP-4115 (COM1) | 8B | User-created cable + RS232C conversion unit by IAI Corporation RCB-CV-MW + Communication cable for PC connection by IAI Corporation CB-ERC2-SIO020 + Power & I/O Cable by IAI Corporation CB-ERC2-PWBIO*** or CB-ERC2-PWBIO***-RB |

*d-4Due to the COM port specifications, flow control is limited, and therefore the wiring diagram may need to be configured differently.
Displays with Limited Support for Control Signals

*2Only the COM port which can communicate by RS-232C can be used.

IPC COM Port

NOTE

- RS232C conversion unit (RCB-CV-MW) and communication cable (CB-ERC2-SIO020) are accessories of PC Interface Software (RCM-101-MW) by IAI Corporation.