### 14A

No. | Name | Notes
--- | --- | ---
(1) | RS232C conversion unit by IAI Corporation RCB-CV-MW |
(2) | Communication cable by IAI Corporation CB-RCA-SIO050 |
(3) | SIO converter by IAI Corporation RC*-TU-SIO-* |
(4) | User-created cable Connector SIO converter side (J4 or J5): e-CON connector (plug) External Device side: MC1.5/4-ST-3.5 (plug) by Phoenix Contact K.K. |

NOTE

- Cable length from SIO converter to External Device: 100m or less