### 5A)

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | COM Port Conversion Adapter by Pro-face CA3-ADPCOM-01 |
(2) | Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 |
(3) | User-created cable Connector Display side: Terminal block External Device side: Terminal block |

NOTE

- Cable length: 500m or less.

- Turn on the DIP Switch for Terminating Resistance Settings on the External Device located at the end.