You can import tag data from the project created by your programming software.

Data Type | Bit Address | Word Address | 32 bit | Notes
--- | --- | --- | --- | ---
BOOL | Single | <TAGNAME> | - | - | *1
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGMNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
BYTE SINT USINT | Single | - | <TAGNAME> |  | *1
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
INT WORD | Single | - | <TAGNAME> | *1
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
DINT UDINT DWORD | Single | - | <TAGNAME> | *1
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
DATE REAL TIME TOD TIME_OF_DAY | Single | - | <TAGNAME> |  | *1
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
DATE_AND_TIME DT | Single | - | <TAGNAME> | - | *1*2
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
STRING | Single | - | <TAGNAME> | - | *1
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
LREAL | Single | - | <TAGNAME> | - |
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
WSTRING | Single | - | <TAGNAME> | - |
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]

*1<TAGNAME>: When referring to structures, the TagName includes the structure name. The maximum number of characters for the Tag Name is 255, which includes delimiters and elements.
Example)
BOOL type single symbol "BOOLSYMBOL"
BOOL type 1D Array "BOOL1D[10]
WORD type 2D Array "WORD2D[10,10]
UDINT type 3D Array "UDINT3D[0,1,2]
STRING in User Defined Structure [STRUCT001] "STRUCT001.STRINGSYM"

*264-bit data type on the Display, 32-bit data type on the External Device.

NOTE

- Export only the required tags from the External Device. If the number of elements of an array exceeds 32768, do not export that array from the External Device.
- Please use the same data type and size in Display corresponding to Tags in External Device.
- For tag import procedures, see the following.
  Importing Symbols from External Devices
- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms