### MP2000 Series / MPU-01

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
System registers | SB000000 - SB08191F | SW00000 - SW08191 |  |
Input registers | IB00000 - IBFFFFF | IW0000 - IWFFFF | *1
Output registers | OB00000 - OBFFFFF | OW0000 - OWFFFF | *1
Data registers | MB000000 - MB65534F | MW00000 - MW65534 |

*1As for Input and Output registers, device 0x9000-0xFFFF cannot be written.

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms