Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) ST6000 2nd Gen*d-4 (COM1) STM6000 (COM1) PC/AT | 1A | 9-pin-to-25-pin RS-232C Conversion Cable by Pro-face CA3-CBLCBT232-01 (0.2m) + Mitsubishi PLC FX Series program control I/F cable by Pro-face GP430-IP11-O (5m) |

*d-4Due to the COM port specifications, flow control is limited, and therefore the wiring diagram may need to be configured differently.
Displays with Limited Support for Control Signals

NOTE

- This cable system cannot be used for connection with GP-4100 series.