### 3I)

Legend | Name | Note
--- | --- | ---
(1) | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 |
(2) | User-created cable Connector Display side: Terminal block External Device side: Terminal block |

NOTE

- To insert termination resistance of 100Ω on the External Device, short-circuit jumper JP2.
- For the External Device connector, use the XH connector (XHP-7) by J.S.T. Mfg.
- Cable length: 500m or less.