*1

Converter output voltage*2

-

S13

Regenerative brake duty

-

-

S14

Electronic thermal relay function load factor

Electronic thermal relay function load factor

-

S15

Output current peak value

Output current peak value

-

S16

Converter output voltage peak value

Converter output voltage peak value

-

S17

Input power

Input power

-

S18

Output power

Output power

-

S19

-

-

-

S20

-

-

-

S21

-

-

-

S22

-

-

-

S23

-

-

-

S24

-

-

-

S25

-

-

-

S26

-

-

-

S27

-

-

-

S28

-

-

-

S29

-

-

-

S30

-

-

-

S31

-

-

-

S32

-

-

-

S33

-

-

-

S34

-

-

-

S35

-

-

-

S36

-

-

-

S37

-

-

-

S38

-

-

-

S39

-

-

-

S40

-

-

-

S41

-

-

-

S42

-

-

-

S43

Alarm definition

(Latest Nos. 1&2)

Alarm definition

(Latest Nos. 1&2)

Alarm definition

(Latest Nos. 1&2)

S44

Alarm definition

(Latest Nos. 3&4)

Alarm definition

(Latest Nos. 3&4)

Alarm definition

(Latest Nos. 3&4)

S45

Alarm definition

(Latest Nos. 5&6)

Alarm definition

(Latest Nos. 5&6)

-

S46

Alarm definition

(Latest Nos. 7&8)

Alarm definition

(Latest Nos. 7&8)

-

S47

-

-

-

S48

Run command

Run command

Run command

S49

-

-

-

S50

Inverter status monitor

Inverter status monitor

Inverter status monitor

S51

Set frequency read (RAM) *1

Set frequency read (RAM)*2

Set frequency read (RAM)

S52

Set frequency read (EEPROM)*1

Set frequency read (EEPROM)*2

Set frequency read (EEPROM)

S53

Set frequency write (RAM)*1

Set frequency write (RAM)*2

Set frequency write (RAM)

S54

Set frequency write (EEPROM)

Set frequency write (EEPROM)

Set frequency write (RAM,EEPROM)

S55

Inverter reset

Inverter reset

Inverter reset

S56

Alarm definition all clear*1

Alarm definition batch clear*2

Alarm definition batch clear

S57

Parameter all clear/User clear

All clear/User clear

All parameter clear

S58

Link parameter expansion setting

Link parameter expansion setting

Link parameter expansion setting

S59

Second parameter changing

Second parameter changing

-

*1Not supported by FR-A500L series. *2Not supported by FR-F500L series.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms