### 11A

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | RS232C conversion unit by IAI Corporation RCB-CV-MW |
(2) | Communication cable by IAI Corporation CB-RCA-SIO050 |
(3) | SIO converter by IAI Corporation RC*-TU-SIO-* |
(4) | Network Connection Cable by IAI Corporation CB-ERC2-CTL001 | Connect to the J4 or J5 on the SIO converter
(5) | Power & I/O Cable by IAI Corporation CB-ERC2-PWBIO*** or CB-ERC2-PWBIO***-RB |

NOTE

- Cable length from SIO converter to External Device: 100m or less

*1 We recommend the IAI Corporation CB-ERC2-PWBIO*** or CB-ERC2-PWBIO***-RB as the Power & I/O Cable.