### 14H

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block RS232C conversion unit side: D-Sub 9 pin (plug) |
(2) | RS232C conversion unit by IAI Corporation RCB-CV-MW |
(3) | Communication cable by IAI Corporation CB-RCA-SIO050 |
(4) | SIO converter by IAI Corporation RC*-TU-SIO-* |
(5) | User-created cable Connector SIO converter side TB1: Link connection terminal block TB2: Power supply and emergency stop terminal block Junction side: e-CON connector (plug) |
(6) | Junction by AMP 5-1473574-4 |
(7) | User-created cable Connector Junction side: e-CON connector (plug) External Device side: MC1.5/4-ST-3.5 (plug) by Phoenix Contact K.K. |
(8) | Termination resistance Connector Junction side: e-CON connector (plug) |

NOTE

- Cable length from SIO converter to External Device: 100m or less