### 4A

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | COM port conversion adapter by Pro-face CA3-ADPCOM-01 |
(2) | Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 |
(3) | Distributor BMJ-8P |
(4) | Distributor BMJ-8 |
(5) | User-created cable (FR-CB20* cable) • Connector Display side: Terminal Block Distributor side: RJ-45 Connector External Device side: RJ-45 Connector |

NOTE

- Total cable length: 500m or less