デバイス | ビットアドレス | ワードアドレス | 32 bit | 備考
--- | --- | --- | --- | ---
BOOL | Single | <TAGNAME> | - | - | ※1
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh] | -
2D Array | <TAGMNAME>[xl,yl] - <TAGNAME>[xh,yh] | -
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh] | -
BYTE SINT USINT | Single | - | <TAGNAME> |  | ※1
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
INT UINT WORD | Single | - | <TAGNAME> | ※1
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
DINT UDINT DWORD | Single | - | <TAGNAME> | ※1
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
DATE REAL TIME TOD TIME_OF_DAY | Single | - | <TAGNAME> | ※1
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
DATE_AND_TIME DT | Single | - | <TAGNAME> | - | ※1
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
STRING | Single | - | <TAGNAME> | - | ※1
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
LINT LWORD ULINT | Single | - | <TAGNAME> | - |
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
LREAL | Single | - | <TAGNAME> | - |
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]
WSTRING | Single | - | <TAGNAME> | - |
1D Array | <TAGNAME>[xl] - <TAGNAME>[xh]
2D Array | <TAGNAME>[xl,yl] - <TAGNAME>[xh,yh]
3D Array | <TAGNAME>[xl,yl,zl] - <TAGNAME>[xh,yh,zh]

※1<TAGNAME>：構造体の場合、構造体名を含んだTag Nameになります。Tag Nameの最大文字数はデリミタ、要素番号を含めて 255文字です。
例）
BOOL type single symbol "BOOLSYMBOL"
BOOL type 1D Array "BOOL1D[10]"
WORD type 2D Array "WORD2D[10,10]"
UDINT type 3D Array "UDINT3D[0,1,2]"
STRING in User Defined Structure [STRUCT001] "STRUCT001.STRINGSYM"

重要:

- EHV+シリーズと接続する場合、配列を表示器に使用することはできません。

MEMO

- 接続機器からは必要なタグのみエクスポートしてください。配列の要素数が 32768を超えた場合、接続機器から配列をエクスポートしないでください。
- サブスコープは 表示器上では'Scope'.'Sub-Scope'. として表示されます('.' はデリミッターです）。
- 接続機器のタグに対応するデータタイプとサイズが同じ表示器のタグを使用してください。
- 表中のアイコンについてはマニュアル表記上の注意を参照してください。
  サポートされているデバイスのシンボルと用語