           3112T WindowsXP drivers installation instructions  (installxp.txt)   8/5/2004 rev 1.1

Driver installation order after a clean installation of the OS:
 1. Chipset driver
 2. Video driver
 3. Lan driver
 4. Audio/Multimedia driver
 5. Touch screen driver

================================================================

Chipset driver installation instructions:

 - Navigate to this products chipset directory on the driver CD.
 - Run sissetup.exe. This will start the AGP wizard.
 - Restart when prompted.

Video driver  installation instructions:

 - Go to the device manager
 - Expand "Display Adapters"
 - Right click on "SiS 300/305/630/540/730"
 - Select "Properties"
 - Select the "driver" tab.
 - Select "update driver"
 - Click Next
 - Click "Finish"
 - Reboot is recommended.

Lan driver  installation instructions:
 - Navigate to the ...\lan\8139C directory on the driver CD.
 - Run setup.exe
 - Click Next
 - Click Finish
 - Reboot is recommended.

Audio/Multimedia driver installation instructions:
 - Go to the device manager
 - Expand the group label Sound, video and game Controller
 - Right click on Sis 7018 Audio Driver
 - Select "properties"
 - Select the "driver" tab
 - Click the  "update driver" button
 - Next
 - Select Version 5.10.0.6150
 - Next
 - Click "Finish"
 - "Power cycle" the system.

Touch screen driver  installation instructions:
 - Navigate to the ...\touch\driver\windows 2000-xp driver v4.01 directory
 - Run the setup.exe.
 - After the setup completes, right click on the PM icon on the lower right toolbar.
 - Select "control panel"
 - Select the "Calibrate" tab
 - Select "standard" calibration
 - Click "OK" after the calibration is complete.
