## Saving the Configuration

After a reset, the Intel® PRO/Wireless 2011B LAN Access Point keeps only configuration changes that were saved.

To make configuration changes permanent:

1. Select Special Functions from the Main Menu .
2. From the Special Functions menu, select Save Configuration and press ENTER . The Save All APs function saves only the five preceding items. The function does not save other configuration parameters. You can perform this option only among the same hardware platforms and firmware versions.
   The Non-Volatile RAM (NVRAM) stores saved configuration information. To clear the NVRAM-stored configuration, see Restoring the Factory Configuration.

Copyright © 2002 Intel Corporation. Legal Information