# Using Intel® PROSet II

Intel® PROSet II enables you to test and configure Intel network adapters. Using the Autorun on the Intel CD, you can install Intel PROSet II on computers running Microsoft Windows* operating systems.

When Intel PROSet II is installed, you'll see two icons as shown below.

System Tray Icon: |
Control Panel Icon: |

Intel PROSet II runs when you click the PROSet II tray icon or the Intel PROSet II icon in the Control Panel (shown below).

The main Intel PROSet II window is similar to this illustration.

If you have a server adapter, you can set the advanced parameters by selecting the desired adapter in the left window and clicking the Advanced tab. To configure teaming features - such as Adapter Fault Tolerance, Adaptive Load Balancing, Fast EtherChannel (FEC), Gigabit EtherChannel (GEC), static 802.3ad Link Aggregation and VLANs - right- click the desired adapter in the left window and follow the teaming wizard. See the Intel PROSet II online help for additional information.

Copyright © 2002 Intel Corporation. Legal Information