## Event History

The access point tracks specific events. The types of events logged are configurable. The log is a 128-entry circular buffer. After the 128th entry, the earliest event entry deletes.

The Event History displays the most recent event at the top of the list. Each event lists a time stamp recorded in hh:mm:ss from the time the access point powered up or reset. The type of event logged follows the time stamp.

## Clearing Statistics

To clear statistics:

1. Select Special Functions from the Main Menu .
2. Select Clear All Statistics . The access point zeroes all statistics.

Resetting the access point also clears statistics.

Copyright © 2002 Intel Corporation. Legal Information